$ EZ-EDS Version 3.23.1.20171205 Generated Electronic Data Sheet

[File]
        DescText = "ET 200SP MF V5.0 Adapter EDS";
        CreateDate = 11-08-2019;
        CreateTime = 12:00:00;
        ModDate = 11-08-2019;
        ModTime = 12:00:01;
        Revision = 1.3;

[Device]
        VendCode = 1251;
        VendName = "Siemens AG";
        ProdType = 12;
        ProdTypeStr = "Communications Adapter";
        ProdCode = 4002;
        MajRev = 50;
        MinRev = 3;
        ProdName = "ET 200SP MF V5.0";
        Catalog = "6ES7 155-6MU00-0CN0";
        Icon = "GSDML-002A-0313-ET200SP-02.ico";
        IconContents =
                "AAABAAEARigQAAEABADoBwAAFgAAACgAAABGAAAAUAAAAAEABAAAAAAAAAAA"
                "AAAAAAAAAAAAEAAAAAAAAAAAAAAAAAC/AAC/AAAAv78AvwAAAL8AvwC/vwAA"
                "wMDAAICAgAAAAP8AAP8AAAD//wD/AAAA/wD/AP//AAD///8A////////////"
                "//////////////////////////////////8A////////////////////////"
                "//////////////////////8A////////////////////////////////////"
                "//////////8A//////////////////////////////////////////////8A"
                "////////////8A////////////////////////////////8A////////////"
                "8A//8AAAAP////////////////////////8A////////////8A//AIiIgP//"
                "//////////////////////8A////////AAAA8A/wgIiIgAAAAAAAAAAAAAAA"
                "AA////////8A///////4CIiA8A8IgIiIgICACACAgAgIAICACA////////8A"
                "//////8ICIiAAACIgIiIgICACACAgAgIAICACA////////8A//////8ICIiA"
                "gACIgIiIgICACACAgAgIAICACA////////8A//////8ICIiAgAAIgIiIgICA"
                "CACAgAgIAICACA////////8A//////8ICIiAgAAIgIiIgICACACAgAgIAICA"
                "CA////////8A//////8ICIiAAAAIgIiIgICACACAgAgIAICACA////////8A"
                "//////8ICIiAAAAIgIiIgICACACAgAgIAICACA////////8A//////8ICIiA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAA//////8A//////8ICIiACIiIiIiAiIgI"
                "iICIiAiIgIiICIiA//////8A//////8ICIgICIiIiIiAqogIiICIiAqogKqI"
                "CIiA//////8A///////wCICICoiIh3dwqogIiICIiAqogKqICIiA//////8A"
                "///////wCICICoiIh3dwqogIiICqiAqogKqICIiA//////8A///////wCICI"
                "CIiIiIiAqogKqICqiAqogKqICqiA//////8A///////wCICICIiIju7g7u4O"
                "7uDu7g7u4O7uDu7g//////8A///////wCICICIiIju7g7u4O7uDu7g7u4O7u"
                "Du7g//////8A///////wCICICIiIju7g7u4O7uDu7g7u4O7uDu7g//////8A"
                "///////wCICICIiIju7g7u4O7uDu7g7u4O7uDu7g//////8A///////wCICI"
                "CIiIju7g7u4O7uDu7g7u4O7uDu7g//////8A//////8ICICICIiIju7g7u4O"
                "7uDu7g7u4O7uDu7g//////8A//////8ICICICIiIiIiAiIgIiICIiAiIgIiI"
                "CIiA//////8A//////8ICICICIiIqJiAqIgKiICoiAqIgKiICoiA//////8A"
                "//////8ICICICIiId3dwd3cHd3B3dwd3cHd3B3dw//////8A//////8ICICI"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAA//////8A//////8ICICAiIiIiIgIiICI"
                "iAiIgIiICIiAiIgP//////8A//////8ICIAIiIiIiICIiAiIgIiICIiAiIgI"
                "iID///////8A//////8IAACIiIiIiAiIgIiICIiAiIgIiICIiA////////8A"
                "//////8AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAP////////8A//////8AAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAD/////////8A////////////////////////"
                "//////////////////////8A////////////////////////////////////"
                "//////////8A//////////////////////////////////////////////8A"
                "//////////////////////////////////////////////8AAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAA";


[Device Classification]
        Class1 = EtherNetIP;


[Params]
        Param9 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0020,                 $ Descriptor
                0xC8,                   $ Data Type
                4,                      $ Data Size in bytes
                "RPI",                  $ name
                "",                     $ units
                "RPI",                  $ help string
                2000,20000000,10000,    $ min, max, default data sizes
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param768 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output Data",          $ name
                "Bytes",                $ units
                "",                     $ help string
                0,246,246,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                0;                      $ decimal places
        Param769 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input Data",           $ name
                "Bytes",                $ units
                "",                     $ help string
                0,500,500,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                0;                      $ decimal places
        Param775 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "Configuration data",   $ name
                "",                     $ units
                "Configuration data",   $ help string
                ,1,1,                   $ min, max, default data sizes
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

[Assembly]
        Object_Name = "Assembly Object";
        Object_Class_Code = 0x04;
        Assem768 =
                "Output",
                "20 04 25 00 00 03 30 03",
                ,
                0x0001,
                ,,
                0,;
        Assem769 =
                "Input",
                "20 04 25 00 01 03 30 03",
                ,
                0x0001,
                ,,
                0,;
        Assem775 =
                "Configuration",
                "20 04 25 00 07 03 30 03",
                ,
                0x0001,
                ,,
                0,;

[Connection Manager]
        Object_Name = "Connection Manager Object";
        Object_Class_Code = 0x06;
				
        Connection1 =
                0x04010002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0xFF64040F,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param9,Param768,Assem768,       $ O->T RPI, size, format
                Param9,Param769,Assem769,       $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,,                      $ target config size, format
                "Connection00 Exclusive",      $ Connection Name
                "Connection00 Exclusive Owner",      $ help string
                "20 04 25 00 07 03 2D 00 00 03 2D 00 01 03";    $ Path

				
[TCP/IP Interface Class]
        Revision = 4;
        Object_Name = "TCP/IP Interface Object";
        Object_Class_Code = 0xF5;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;

[Ethernet Link Class]
        Revision = 4;
        Object_Name = "Ethernet Link Object";
        Object_Class_Code = 0xF6;
        MaxInst = 2;
        Number_Of_Static_Instances = 2;
        Max_Number_Of_Dynamic_Instances = 0;
        InterfaceLabel1 = "X1 P1";
        InterfaceLabel2 = "X1 P2";

