{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["24V","480V"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"24V","index":0,"n_rows":13,"n_cols":17,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Hersteller","Artikelnummer","Link","Bustyp","Nennstrom in A","Kanäle max.","Status tripped","Spannungsmessung","Strommessung","Auslösestrom in A","Periode in ms","Bytes zyklisch",null,null,"Untermodule","Zusatzmodule"]
[null,"Block","EB-IO-LINK","https://www.block.eu/de_DE/produktvariante/eb-io-link/","IO-Link",40,"40x1","zyklisch","azyklisch","azyklisch 16bit","fest od. variabel 0,5/1/2/3/4/5/6/8/10",2,6,null,null,"EB-0824-xxx-0","EB-GNDx"]
[null,"Block","EB-IO-LINK1","https://www.block.eu/de_DE/produktvariante/eb-io-link1/","IO-Link",40,"16x1","zyklisch","azyklisch","zyklisch 8bit + azyklisch 16bit","fest od. variabel 0,5/1/2/3/4/5/6/8/10",2,23,null,null,"EB-0824-xxx-0","EB-GNDx"]
[]
[null,"Wago","787-1668/000-080","https://www.wago.com/de/stromversorgungen/elektronischer-schutzschalter/p/787-1668_006-1000","IO-Link",{"$f":"8*10","v":80},"1x8","zyklisch","azyklisch 100mV acc.","azyklisch 100mA acc.","variabel 1/2/3/4/6/8",null,5,null,null,"-"]
[]
[null,"Rockwell","1694-PFD1244","https://www.rockwellautomation.com/de-at/products/hardware/allen-bradley/circuit-and-load-protection/electronic-circuit-protection-modules/1694-electronic-circuit-protection.html","IO-Link",40,"16x1 / 16x2","zyklisch","azyklisch 10mV acc.","zyklisch 100mA acc.","fest 1/2/3/4/6/8/10  od. variabel 1A inc.","(s. Rockwell Studio)",null,null,null,"1694-PMD2A10"]
[null,null,null,"https://ideadigitalasset.com/DAMRoot/Original/10782/11994_E2O7T5KVAYZ0CSMW.pdf","IO-Link",{"$nulls":7},"2? / 44?"]
[]
[null,"E-T-A","ControlPlex® DINrail EM12D-TIO","https://www.e-t-a.de/produkte/intelligente_stromverteilung/controlplex/controlplex_dinrail/controlplex_dinrail_em12d_tio/","IO-Link",40,"16x1 / 8x2",null,null,null,"fest 1/2/3/4/6 od. variabel 1-4 / 1-10",{"$nulls":4},"REX12D-TE2-100-DC24V-1A-10A","EM12-T00-100-LINE-40A"]
[null,"E-T-A","ControlPlex® System CPC12 ","https://www.e-t-a.de/produkte/intelligente_stromverteilung/controlplex/controlplex_dinrail/controlplex_system_cpc12_profinet_ethercat_ethernetip_modbus_tcp/","PROFINET, EtherCAT, EtherNET/IP, Modbus TCP",40,{"$nulls":4},"fest 1/2/3/4/6 od. variabel 1-4 / 1-10",{"$nulls":4},"REX12D-TE2-100-DC24V-1A-10A","EM12-T00-100-LINE-40A"]

{"sheet":"480V","index":1,"n_rows":14,"n_cols":17,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[null,null,"Energy Meters"]
[]
[null,"Hersteller","Artikelnummer","Link","Bustyp","Nennstrom in A","Nennspannung","Datenspeicher","Erfasste Messwerte",{"$nulls":6},"Untermodule","Zusatzmodule"]
[null,"Schneider Electric","EM3550","https://www.se.com/de/de/download/document/PLSED310037EN_Web/","Modbus RTU","20 - 5000","600V AC","10x 16-bit Data Buffers","I, U, P, Q, S, E, ∑I, ∑P, f, PF, THD…",null,"Energiemonitor",{"$nulls":4},"METSECTR25500"]
[null,"Mitsubishi","EMU4-HD1-MB","https://www.mitsubishielectric.com/fa/products/pmng/ems/pmerit/ecomonitor/ecomonitor_Light_2.html","Modbus RTU / Modbus TCP / CC-Link / CC-Link IE","50 - 600","480V AC",null,"I, U, P, Q, S, E, ∑I, ∑P, f, PF, THD…",null,"Energiemonitor",{"$nulls":4},"EMU-CT250-A"]
[null,"Siemens","7KT PAC1200","https://mall.industry.siemens.com/mall/en/de/Catalog/Products/10289825?activeTab=ProductInformation#Application","?, LAN/IP","40 / 63","?","2GB","E, Q, f, P",null,"multichannel current measuring",{"$nulls":4},"7KT1238","7KT1260"]
[]
[]
[]
[]
[]
[null,"Hager","h3+","https://www.hager.ch/loesungen/zweckbau/schutzgeraete/leistungsschalter-h3+/423497.htm","Modbus RTU","25 - 250",null,null,"I, U, P, Q, S, E, ∑I, ∑P, f, PF, THD…",null,"Leistungsschalter"]
[null,"Eaton","NZM2 PXR25","https://datasheet.eaton.com/datasheet.php?model=192145&locale=de_DE","Modbus RTU",100,"690V AC",null,"?",null,"Leistungsschalter"]
[null,"Siemens","3WA","https://new.siemens.com/de/de/produkte/energie/niederspannung/komponenten/sentron-schutzgeraete/offene-leistungsschalter-3wa.html","?",null,"?",null,"?",null,"Leistungsschalter"]