{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":5,"n_cols":17,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[null,null,"Energy Meters"]
[]
[null,"Hersteller","Artikelnummer","Link","Bustyp","Nennstrom in A","Nennspannung","Datenspeicher",{"$nulls":7},"Untermodule","Zusatzmodule"]
[null,"Schneider Electric","EM3550","https://www.se.com/de/de/download/document/PLSED310037EN_Web/","Modbus RTU","20 - 5000","600V AC","10x 16-bit Data Buffers",{"$nulls":7},"METSECTR25500"]
[null,"Mitsubishi","EMU4-HD1-MB","https://www.mitsubishielectric.com/fa/products/pmng/ems/pmerit/ecomonitor/ecomonitor_Light_2.html","Modbus RTU / Modbus TCP / CC-Link / CC-Link IE","50 - 600","480V AC",{"$nulls":8},"EMU-CT250-A"]