{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":34,"n_cols":12,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Windkanalsteuerung",null,null,null,"Bill of Materials"]
[]
[]
[]
[null,"Designator","Name",null,null,"Footprint","Stück",null,"Wert",null,"Preis","Link"]
["Passiv"]
[null,"C1,C6,C2,C5","SMD Kondensator",null,null,"0805'",4,null,"100n-10u",null,{"$f":"4*0.279","v":1.1160000000000001},"https://www.mouser.de/ProductDetail/KEMET/C0805C105M8RACAUTO?qs=sGAEpiMZZMsh%252B1woXyUXj5pr%2Fm5%2FLKZI74TXDpZxCL0%3D"]
[null,"R2,R3,R4,R5,R5,R7,R8","SMD Widerstand",null,null,"0805'",7,null,"1k",null,{"$f":"0.654*7","v":4.5780000000000003},"https://www.mouser.de/ProductDetail/KOA-Speer/RN73H2ATTD1001B25?qs=sGAEpiMZZMvdGkrng054t6r%2FWflXw%252BJyf2SUOj2tzAM%3D"]
[null,"R1","SMD Widerstand",null,null,"0805'",1,null,"270 Ohm",null,{"$f":"0.117","v":0.11700000000000001},"https://www.mouser.de/ProductDetail/ROHM-Semiconductor/KTR10EZPJ271?qs=sGAEpiMZZMvdGkrng054t621aZ%2Fa1rARVpBt83haE4BjzCWz5wSBVA%3D%3D"]
["Aktiv"]
[null,"LED1","Led Grün",null,null,"5mm",1,null,null,null,0.23,"https://www.mouser.de/ProductDetail/Kingbright/WP7113SGD?qs=sGAEpiMZZMtmwHDZQCdlqVL6rcvtIz013ClYTS5m%2F8c%3D"]
[null,"LED2","LED Rot",null,null,"5mm",1,null,null,null,0.432,"https://www.mouser.de/ProductDetail/Kingbright/WP57IID?qs=sGAEpiMZZMtmwHDZQCdlqS%252B42B3%252BlPHXk7xWDmOie50%3D"]
[null,"LED3","LED Gelb",null,null,"5mm",1,null,null,null,0.41,"https://www.mouser.de/ProductDetail/Kingbright/WP57YYD?qs=sGAEpiMZZMtmwHDZQCdlqS%252B42B3%252BlPHXES7nvRsxVpA%3D"]
[null,"Q1,Q4","SMD NPN Transistor",null,null,"SOT-23",2,null,"MMBT5551",null,{"$f":"2*0.162","v":0.32400000000000001},"https://www.mouser.de/ProductDetail/ON-Semiconductor/MMBT5551LT1G?qs=sGAEpiMZZMutXGli8Ay4kC402l06AIhPcyRrZFuJbVk%3D"]
[null,"Q2","SMD PNP Transistor",null,null,"SOT-23",1,null,"MMBT5401",null,0.153,"https://www.mouser.de/ProductDetail/ON-Semiconductor/MMBT5401LT1G?qs=sGAEpiMZZMutXGli8Ay4kK2TqWlAzC1zwHYVH5ZeC0k%3D"]
["ICs"]
[null,"U2,U5","8-Kanal SPI ADC",null,null,"SOIC-16",2,null,"MCP3008-ISL",null,{"$f":"2*1.97","v":3.94},"https://www.mouser.de/ProductDetail/Microchip-Technology/MCP3008-I-SL?qs=sGAEpiMZZMvTvDTV69d2Qh8oAuXtCOKDL2vySlNGbrs%3D"]
[null,"U4","Bidirektionaler Pegelwandler",null,null,"SSOP-20",1,null,"IC_TXB0108PW",null,1.36,"https://www.mouser.de/ProductDetail/Texas-Instruments/TXB0108PWR?qs=sGAEpiMZZMupTq4AYuRvQKKOVTxKvBsp"]
["Mechanisch"]
[null,"JP1-JP7","Zweifach-Schraubklemme",null,null,"3,5mm pitch",15,null,null,null,{"$f":"15*0.66","v":9.9},"https://www.mouser.de/ProductDetail/Wurth-Elektronik/691214110002?qs=sGAEpiMZZMvZTcaMAxB2AHc%2Flkca1rcTw%252BBy6B6lIsB%2FttEijmIyBA%3D%3D"]
[null,"P1","2x20-pin stackable Header",null,null,"2,54mm pitch",1,null,null,null,2.66,"https://www.mouser.de/ProductDetail/SparkFun/PRT-12790?qs=sGAEpiMZZMuM1nRwI3zz2UpCr55iWBr5lB8eP%252BN21iPCXuFC0LpVqw%3D%3D"]
[null,"H1","1x3-pin stackable Header",null,null,"2,54mm pitch",1,null,null,null,0.46800000000000003,"https://www.mouser.de/ProductDetail/SparkFun/PRT-13875?qs=sGAEpiMZZMuM1nRwI3zz2UpCr55iWBr5BBnap2GnHlTbAo3MoTe6Ew%3D%3D"]
["PCB"]
[null,"für die meisten Anbiebter als Gerber exportierbar",null,null,null,"65mm x 65mm",{"$nulls":5},"https://easyeda.com/User201/windkanal"]
["Sonstige"]
[null,"Banana Pi BPI-M2+","Single-Board-Computer",null,null,null,1,null,null,null,53.99,"https://www.conrad.de/de/p/banana-pi-bpi-m2-1-gb-4-x-1-0-ghz-banana-pi-1435682.html"]
[null,"M2.5 Abstandshalter für PI und PCB",null,null,null,"M2.5, 10mm",4]
[null,"Netzteil","5V 3A",null,null,null,1,null,"(bereits vorhanden)"]
[null,"HDMI Verlängerungskabel zum Einbau",null,null,null,"1m",1,null,"(falls gewünscht)",null,11.99,"https://www.conrad.de/de/p/hdmi-verlaengerungskabel-zum-einbau-1x-hdmi-stecker-1x-hdmi-buchse-1-m-schwarz-delock-1421657.html"]
[null,"USB Verlängerungskabel zum Einbau",null,null,null,"0,5m",2,null,"(falls gewünscht)",null,{"$f":"8.49*2","v":16.98},"https://www.conrad.de/de/p/delock-usb-2-0-anschlusskabel-1x-usb-2-0-stecker-a-1x-usb-2-0-buchse-a-0-5-m-schwarz-vergoldete-steckkontakte-1651192.html"]
[]
[{"$nulls":10},{"$f":"SUM(K9:K32)","v":108.648}]