{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":14,"n_cols":17,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[null,null,"Energy Meters"]
[]
[null,"Hersteller","Artikelnummer","Link","Bustyp","Nennstrom in A","Nennspannung","Datenspeicher","Erfasste Messwerte",{"$nulls":6},"Untermodule","Zusatzmodule"]
[null,"Schneider Electric","EM3550","https://www.se.com/de/de/download/document/PLSED310037EN_Web/","Modbus RTU","20 - 5000","600V AC","10x 16-bit Data Buffers","I, U, P, Q, S, E, ∑I, ∑P, f, PF, THD…",null,"Energiemonitor",{"$nulls":4},"METSECTR25500"]
[null,"Mitsubishi","EMU4-HD1-MB","https://www.mitsubishielectric.com/fa/products/pmng/ems/pmerit/ecomonitor/ecomonitor_Light_2.html","Modbus RTU / Modbus TCP / CC-Link / CC-Link IE","50 - 600","480V AC",null,"I, U, P, Q, S, E, ∑I, ∑P, f, PF, THD…",null,"Energiemonitor",{"$nulls":4},"EMU-CT250-A"]
[null,"Siemens","7KT PAC1200","https://mall.industry.siemens.com/mall/en/de/Catalog/Products/10289825?activeTab=ProductInformation#Application","?, LAN/IP","40 / 63","?","2GB","E, Q, f, P",null,"multichannel current measuring",{"$nulls":4},"7KT1238","7KT1260"]
[]
[]
[]
[]
[]
[null,"Hager","h3+","https://www.hager.ch/loesungen/zweckbau/schutzgeraete/leistungsschalter-h3+/423497.htm","Modbus RTU","25 - 250",null,null,"I, U, P, Q, S, E, ∑I, ∑P, f, PF, THD…",null,"Leistungsschalter"]
[null,"Eaton","NZM2 PXR25","https://datasheet.eaton.com/datasheet.php?model=192145&locale=de_DE","Modbus RTU",100,"690V AC",null,"?",null,"Leistungsschalter"]
[null,"Siemens","3WA","https://new.siemens.com/de/de/produkte/energie/niederspannung/komponenten/sentron-schutzgeraete/offene-leistungsschalter-3wa.html","?",null,"?",null,"?",null,"Leistungsschalter"]